Flashing Firmware:

Step 1: Download firmware .bin file included in this zip folder

Step 2: Download QMK Toolbox for your computer. It is available here: <https://github.com/qmk/qmk_toolbox/releases>

Step 3: Make sure the Bluetooth switch on the back of the keyboard is in "Off" position

Step 4: Open QMK Toolbox and connect the USB cable to a port on your computer. Please make sure that the USB-C side is not connected to the keyboard

Step 5: Press down on the "ESC" key on the WhiteFox Eclipse. While keeping "ESC" pressed down, plug in the USB cable into the USB-C port of the keyboard. QMK Toolbox will recognize the keyboard in flashing mode and should show text in yellow color

Step 6: Select the firmware file in QMK toolbox and press "Flash"

Loading Default Layout on WhiteFox Eclipse using VIA Configurator:

Step 1: Connect WhiteFox Eclipse to your computer with the USB cable. Make sure Bluetooth switch at the back of the keyboard is turned off

Step 2: Go to <https://usevia.app/>

Step 3: Press “Authorize”. You see a prompt with WhiteFox Eclipse shown. Select the keyboard and press “Pair”

Step 4: Press “Floppy Disk” icon

Step 5: Choose “Load Saved Layout” and load the JSON File included in this zip folder

Please message [help@projecteclipse.co](mailto:help@projecteclipse.co) if any more information is required on the above steps