Tender document

Part number:
BWNC-442FBIF

Kurzbeschreibung:
bullet camera with fixed lens 2.8mm
H.265(+), 120dB TrueWDR, PoE, SmartIR

Technical specifications:
Type : IP Day/Night IR bullet camera
Decoding / Video / Lens : >>>>>DECODING/VIDEO/LENS<<<<<
Sensor type : 1/3" Progressive Scan CMOS
Effective pixel : 2688(H) x 1520(V)
Max. Picture resolution (pixel) : 4MP(2688x1520)/2MP(1920x1080) / 1MP(1280x720)
Video codec : H.264, H.264+, H.265,  H.265+, MJPEG(Substream)
Streaming Method : Unicast / Multicast
Max frame rate mainstream : 25/30fps at 4MP
Max frame rate 1.sub stream : 25 fps at D1
Max frame rate 2.sub stream : 25 fps at 720P
Bit Rate Control : CBR / VBR
Bit Rate per channel : H.264: 24-10240Kbps ; H.265: 14-9984Kbps
Number of video streams : 3 (individually adjustable)
Lens mount : Intern
Lens type : Fixlens
Focal length : 2,8mm
Optical zoom : -
Angle of view (horizontal) : 103°
Angle of view (vertical) : 55°
Sensitivity (Lux) : 0,005 Lux, F1.6 (color)
Sensitivity (Lux) : 0 Lux, F1.6 (IR on)
S/N ratio (dB) : >50 dB
IR cut filter : ICR-IR-Cut filter
Shutter (sec.) : 1/3 - 1/10000
DETECT-OBSERVE-RECOGNIZE-IDENTIFY : >DETECT-OBSERVE-RECOGNIZE-IDENTIFY<
DORI max. (Detect-Observe-Recognize-Identify) : 57m  -  23m  -  11m  -  6m
Features : >>>>>>>>>>FEATURES<<<<<<<<<<<
Digital zoom : 16x
Day/night mode adjustment : Auto (ICR) / color / B/W
Automatic gain control (AGC) : AGC, manual
Digital noise reduction (DNR) : 2NR / 3DNR
White balance : Auto/Natural/Street Lamp/Outdoor/Manual
Backlight compensation : BLC, HLC, TrueWDR(120dB)
Wide dynamic range (WDR) : 120 dB WDR (True WDR)
Mirroring (vertical) : Yes
Picture flip (horizontal) : Yes
Camera title : Yes
Privacy zones : Yes, 4 zones
Region of Interest (ROI) : Yes, 4 zones
ANR (automatic network reproduction) : Yes (for records)
Video analysis : >>>>>>>>Videoanalytics<<<<<<<<<
Motion detection : Yes, 4 areas
Tampering Alarm : Yes
Scene change (tampering) : Yes
IVA via ONVIF Motion : Yes
Tripwire (IVA) : Yes
Intrusion (IVA) : Yes
AI Analytics : Car, Human
Interface : >>>>>>>>>INTERFACE<<<<<<<<<
Audio in-/outputs : -
Audio codec : -
Alarm contacts I/O : 0 / 0
Relay type (output) : -
SD-card slot : Yes, max. 256GB (optional)
Network : >>>>>>>>>>NETWORK<<<<<<<<<<<
Ethernet connector : RJ-45
Ethernet standards : 10/100Base-T
Ethernet speed : 10 / 100 Mbit
PoE standard : IEEE 802.3af
POE CLass : 0
ePoE / Long-Range-PoE : No
Remote : >>>>>>>>>>>REMOTE<<<<<<<<<<<
Max number of users : 10
Alarm management : HTTP, FTP, SMTP, ONVIF,NAS(NFS)
Schedule : Yes
Management software support : Many VMS
Supported browser : Internet Explorer 11, Chrome, Firefox, (Safari)
P2P support : Yes
Cloud service : Yes, BURG-WÄCHTER cloud
Smartphone App : BurgCam App
Push-Notification : Yes, BURGcam PRO App
Security features : HTTPS, SSH, IP Filter
Supported protocols : HTTP,HTTPS,FTP,TCP,UDP, DHCP, SSH,NTP,ONVIF...
Supported software standards : ONVIF, PSIA, CGI
ONVIF version/profile : ONVIF Profile S&G&T
Edge Recording : NAS(NFS), locall PC, micro SD card,FTP
General : >>>>>>>>>>GENERAL<<<<<<<<<<
Classification : IP-67
Vandal-proof : Yes, acc. to IK10
Installation : Wall mount, ceiling mount and pole mount
Camera mounting : Screw mounting
Housing colour : White
Housing material : Aluminium
Integrated IR-LEDs : Yes
Wavelength LED : 850 nm
IR distance (m. ca.) : 30
Smart IR : Yes
Voltage : 12 VDC (+/-25%), PoE
Max. Power consumption (watt) : 5,4 (IR on)
Operating temperature (°C) : -30 to +60
Storage temperature (°C) : 0 to +60
Rel. humidity (%) : Max. 95, non-condensing
Dimensions ØxH (mm) : 55 x 109
Weight : 0,59 kg
Identifier : CE
Items included in delivery : Quick install guide, screws+anchors
Items included in delivery : Mounting drawing paper, LAN cable water prot.
Specials : H.265,AI IVA, TrueWDR(120dB)