Signal Box

Always “dry run” parts before gluing with a woodwork quality PVA.

Start with the longer ground floor and place the MDF on a flat surface.

Glue on the brick engraved 3mm walls and once dry, glue the 3mm thick “combs” inside the top edges (fingers pointing outwards) this assembly supports the balcony.

 Ensure the balcony supports are square then set aside to dry.

Glue the railings into the tabs along the balcony and once dry glue this assembly onto the brick walls and balcony supports.

Glue the 4 internal walls to the 1st floor. Once dry, prime and paint as required.

It is recommended that the outer cladding 2mm walls are primed and painted **before gluing on.**



Glue the “zig zag” strip to the inside of the stair railings, check to align the bottom tag and ensure the 3 slots are aligned.

Once railings strips have dried, starting at the top end, glue in the jointed step. Glue the remaining two jointed steps, middle step followed by the bottom step whilst wet, glue on the second railing piece. Again, work from top to bottom, the natural flex of the 2mm MDF will allow you to bend the last piece to fit. Check this sub assembly is square and set aside to partially dry.

Complete the stairway by gluing the remaining plain steps. Continue to work from top to bottom. Once dry, glue the bottom two tags into the slots on the base and affix to the balcony. Glue each of the vertical posts at the top of the stairs to the railings running along the edge of the balcony.

****

.

Glue the two engraved roof sections to the two triangular gables and when dry, glue in a rectangular locating piece on the inside of each end. Ensure the locating piece protrudes approximately 5 mm for best results.

Cut the ½ round plastic strip into 8-10mm lengths and glue along the apex of the roof to cover the seam.

 ****

Turn the 1st floor over and glue on a locating block in the rear corner diagonally opposite from the balcony. This 3mm corner piece will locate the top floor during use.

Paint the 3 “sliding” windows and doors before gluing into the fully painted model.

**Thank you for buying this kit from**

**Charlie Foxtrot Models** [**www.charliefoxtrotmodels.com**](http://www.charliefoxtrotmodels.com)