A close up of a sign

Description automatically generatedDirt Warrior Accessories – POLARIS RANGER

Front Windshield

**Helpful Hints for Installation:**

*Tools Needed:*

* *![A picture containing indoor, wall

  Description automatically generated]()Phillips #3 Screwdriver or Screw tip for Screw Gun*
* *7/16” Socket or wrench*
* First remove “S” clips and brackets from window (if they came attached to window) See Diagram on back page: This windshield has (2) S clips and (2) brackets.

**PIC 1A**

**pic
**Hold windshield up and lay in place on cage. It should sit inside grooves on the pro-fit cage. This step usually works best with 2 people

* **A picture containing text, vehicle, curb

  Description automatically generated**With screws, washers, and nuts (supplied & shown in pic) Place S clip in slot of cage as shown in Pic 1C.

Windshield Aluminum Frame HereThis end fits in the slot on the Pro-fit cage

**PIC 1B**

* Next, attach brackets to windshield first and then to roll cage. The end with 2 holes mounts to the windshield and the end with 1 hole mounts to the roll cage. You do not have to drill, there is a hole in the cage from the factory that you will use. (See diagram on back page for placement)

**PIC 1D**

**PIC 1C**

* Next, position window so that it is high enough for the vents to open but close enough to the hood that you get a tight fit. Then, position side to side to center window on roll cage.
* Once you have the window positioned, begin tightening all screws.
* Now that the window is on, verify that the vent flaps operate correctly.

**Thank YOU for your BUSINESS & Have A DiRtY DAY!!!**

**Diagram

Description automatically generated**