Kassalade CD350

Metaal

**910181 - 6V output**

**910182 - 12V output**

* Metal cash drawer.
* RJ11 connector ( telephonic type).
* 8 compartments for coins, adjustable in width.
* 4 compartments for banknotes, adjustable in width, with metal pieces to fix banknotes.
* Black colour.
* Frontal slot for cash transactions when not paying in cash or using big banknotes.
* Lock in the frontal part of the box to be opened manually.
* Compatible with RTI / RTN / STI (CD350-6V).
* Compatible with S70 (CD350-12V).

