

upgrade steps


1. Unzip the software package,

Double-click to open the M32 BootLoader\_180724 upgrade tool.




2.Click Open Device Code Hex 

3.Select the HEX upgrade file.



4.Press FN+delete to switch the keyboard to wired mode, and ignore this item if it is already in wired mode.

5.Click Bum Device Code to upgrade.



6.upgrade completed successfully

