Forklift Answer Key #2

|  |  |  |  |
| --- | --- | --- | --- |
| Instructor: |  | Name: |  |
| Class: |  | Date: |  |
| Time: |  | Results: |  |

Instructions

Read each question carefully and mark the correct answer. If you have any questions, raise your hand and the instructor will assist you.

1. An employee must be at least **18** years old to operate a forklift.
2. What does the E type designation on a forklift mean?
   1. It can be used indoors or outdoors.
   2. **It is electrically powered.**
   3. It is diesel fuel powered.
   4. It is safe to use in hazardous atmospheres.
3. When the center of gravity is inside the stability triangle, the load is stable.

**True** False

1. Forklifts must be certified by ANSI and marked as such. **True** False
2. Forklift modifications must be:
   1. **Approved in writing by the manufacturer.**
   2. Just approved by management.
   3. Made by the operator as long as they do not affect vehicle stability.
   4. Made by a competent person.
3. The trucks resistance to turning over sideways is known as its:
   1. Center of gravity.
   2. Turn resistance.
   3. **Lateral stability.**
   4. Dynamic stability.
4. Forklifts must have overhead guards to protect operators from falling objects.

**True** False

1. Operators must wear seatbelts. **True** False
2. What should you do if you are seated in a forklift and it tips over?

**Remain seated and lean away from the direction of the fall.**

1. Which direction should you face when entering or exiting a powered industrial truck?

**Face the vehicle.**

1. Forklifts may not be parked within **8** feet of railroad tracks.
2. Forklifts must maintain at least **three**  vehicle lengths from the forklift ahead.
3. Why is it important to make slow and controlled turns?

**Turning to quickly can affect vehicle stability and cause it to tip over.**

1. What special precautions must be taken for loading or unloading highway trucks?

**The brakes must be set and the rear wheels must be chocked.**

1. Fuel tanks may be filled while the forklift engine is running. True **False**